When updating the screen firmware, please connect the keyboard using a USB cable and switch it on. Once the update is complete, switch the keyboard off and on again, then unplug and reinsert the keyboard.
